0 / 1 point

An \_\_\_\_\_\_\_\_\_ authenticator is an access point or NAS that requires EAP authentication prior to granting access to a network.

Incorrect answer:

EAP authenticator

Correct Answer:EAP

**Results for question 2.**

2

0 / 1 point

In effect, \_\_\_\_\_\_\_\_ is an operating system in the cloud.



DHCP

, Not Selected



PaaS

, Not Selected



IEEE 802.1X

, Not Selected

Incorrect answer:



IaaS

Correct Answer:

PaaS

**Results for question 3.**

3

0 / 1 point

A \_\_\_\_\_\_\_\_\_ is an entity at one end of a point-to-point LAN segment that seeks to be authenticated by an authenticator attached to the other end of that link.

Incorrect answer:

Supplicant

Correct Answer:supplicant

**Results for question 4.**

4

0 / 1 point

The \_\_\_\_\_\_\_\_\_\_\_ functions as an access control point for users in remote locations connecting to an enterprise’s internal network.

Incorrect answer:

network access server

Correct Answer:Network access server, NAS

**Results for question 5.**

5

1 / 1 point

For many clients, the most devastating impact from a security breach is the loss or leakage of data.

Correct answer:

True

False

**Results for question 6.**

6

1 / 1 point

\_\_\_\_\_\_\_\_\_ is the provision of security applications and services via the cloud either to cloud-based infrastructure and software or from the cloud to the customers’ on-premise systems.



IaaS

, Not Selected



PaaS

, Not Selected

Correct answer:



SecaaS



SaaS

, Not Selected

**Results for question 7.**

7

1 / 1 point

A \_\_\_\_\_\_\_\_\_ is a person or organization that maintains a business relationship with, and uses service from, cloud providers.

Correct answer:



cloud consumer



cloud auditor

, Not Selected



cloud broker

, Not Selected



cloud carrier

, Not Selected

**Results for question 8.**

8

1 / 1 point

\_\_\_\_\_\_\_\_\_ saves the complexity of software installation, maintenance, upgrades, and patches.



EAP

, Not Selected

Correct answer:



SaaS



IaaS

, Not Selected



DHCP

, Not Selected

**Results for question 9.**

9

1 / 1 point

\_\_\_\_\_\_\_\_\_ defines how the TLS protocol can be encapsulated in EAP messages.

Correct answer:

EAP-TLS

**Results for question 10.**

10

1 / 1 point

Data must be secured while at rest, in transit, and in use, and access to the data must be controlled.

Correct answer:

True

False

The threat of data compromise decreases in the cloud.

True

Correct answer:

False

### Results for question 2.

2

1 / 1 point

\_\_\_\_\_\_\_\_\_\_\_ is an umbrella term for managing access to a network.

Correct answer:



NAC



RAS

, Not Selected



ARC

, Not Selected



NAS

, Not Selected

### Results for question 3.

3

1 / 1 point

\_\_\_\_\_\_\_\_\_ is a client computer that is attempting to access a network.



NAC

, Not Selected



RAS

, Not Selected

Correct answer:



EAP peer



PSK

, Not Selected

### Results for question 4.

4

1 / 1 point

The cloud provider in a private cloud infrastructure is responsible for both the infrastructure and the control.

True

Correct answer:

False

### Results for question 5.

5

1 / 1 point

An \_\_\_\_\_\_\_\_\_\_ server is a server computer that negotiates the use of a specific EAP method with an EAP peer, validates the EAP peer’s credentials, and authorizes access to the network.

Correct answer:

authentication

### Results for question 6.

6

1 / 1 point

The \_\_\_\_\_\_\_\_\_\_ is an Internet protocol that enables dynamic allocation of IP addresses to hosts.



VLAN

, Not Selected



IEEE 802.1X

, Not Selected

Correct answer:



DHCP



EAPS

, Not Selected

### Results for question 7.

7

1 / 1 point

\_\_\_\_\_\_\_\_\_ saves the complexity of software installation, maintenance, upgrades, and patches.

Correct answer:



SaaS



EAP

, Not Selected



IaaS

, Not Selected



DHCP

, Not Selected

### Results for question 8.

8

1 / 1 point

The \_\_\_\_\_\_\_\_\_\_ determines what access should be granted.



authentication server

, Not Selected



access requestor

, Not Selected

Correct answer:



policy server



supplicant

, Not Selected

### Results for question 9.

9

1 / 1 point

There is a decreasing trend in organizations to move information technology operations to a cloud computing infrastructure.

True

Correct answer:

False

### Results for question 10.

10

1 / 1 point

A \_\_\_\_\_\_\_\_\_\_ provides a form of NAC by allowing or denying network traffic between an enterprise host and an external user.

Correct answer:

Firewall

In using cloud infrastructures, the client necessarily cedes control to the CP on a number of issues that may affect security.

Correct answer:

True

False

### Results for question 2.

2

1 / 1 point

\_\_\_\_\_\_\_\_\_ is a client computer that is attempting to access a network.



RAS

, Not Selected



NAC

, Not Selected



PSK

, Not Selected

Correct answer:



EAP peer

### Results for question 3.

3

1 / 1 point

A cloud broker is useful when cloud services are too complex for a cloud consumer to easily manage.

Correct answer:

True

False

### Results for question 4.

4

1 / 1 point

EAPOL operates at the network layers and makes use of an IEEE 802 LAN, such as Ethernet or Wi-Fi, at the link level.

Correct answer:

True

False

### Results for question 5.

5

1 / 1 point

A \_\_\_\_\_\_\_\_\_ is a person or organization that maintains a business relationship with, and uses service from, cloud providers.



cloud carrier

, Not Selected



cloud auditor

, Not Selected

Correct answer:



cloud consumer



cloud broker

, Not Selected

### Results for question 6.

6

1 / 1 point

A network access server does not include its own authentication services.

True

Correct answer:

False

### Results for question 7.

7

1 / 1 point

VLANs are common NAC enforcement methods.

Correct answer:

True

False

### Results for question 8.

8

1 / 1 point

A \_\_\_\_\_\_\_\_\_\_ provides a form of NAC by allowing or denying network traffic between an enterprise host and an external user.

Correct answer:

firewall

### Results for question 9.

9

1 / 1 point

The \_\_\_\_\_\_\_\_\_ is the node that is attempting to access the network and may be any device that is managed by the network access control system.



RAS

, Not Selected

Correct answer:



AR



IP

, Not Selected



PS

, Not Selected

### Results for question 10.

10

1 / 1 point

In effect, \_\_\_\_\_\_\_\_ is an operating system in the cloud.



IaaS

, Not Selected

Correct answer:



PaaS



DHCP

, Not Selected



IEEE 802.1X